## Radio Buttons

The radio buttons do not affect the input data but only control the format of the displayed results. There are four groups of radio buttons: the Power Unit radio-box in the main window and one radio-box on each page of the bottom tabbed container.

Power Unit Radio-Box

Clicking a button in the Power Unit radio-box affects the following quantities:

- In the main window: Power values in the Magnetron Output group.

- In the Transmission tabsheet: All values in the Incident Power, Reflected Power, and Absorbed Power rows.

- In the Power Meas tabsheet:

- The values in the True Value column.

- If the Error Unit radio-box is set to = P Unit, all the remaining values are also affected.

Unit Radio-Box on Transmission Page

The Unit radio-box in the Transmission tabsheet affects the values in the Interference Factor and Transducer Gain rows.

Error Unit Radio-Box on Power Meas Page

If the Error Unit radio-box is set to = P Unit, then format of all displayed powers is equal to that selected in the Power Unit radio-box of the main window.

Otherwise, only the True Value column format is determined by Power Unit radio-box; the format of the remaining (Min and Max) displays is defined by the Error Unit radio-box.